Title: Gantry Crane Training Certification
Author: G52-ga-172
Last saved by: sdelfante
Company: UWA

FORM 14(b)

Gantry Crane and Lifting Hoist TRAINING RECORD

Name:

Position:

Student Number:
		
Date:
		
Contact Details:			

TRAINING CHECK LIST

1.	Safe Operation of the Thermodynamics Laboratory 1000 kg Gantry Crane

1)	Safe use of slings and chains

2)	Safe positioning of personal when attempting a lift

3)	Use of ‘pull lines’ when guiding a load

4)	Checking the condition of lifting equipment and SWL ratings.

2.	Safety guidelines for the Thermodynamics Laboratory 1000 kg Gantry Crane

1)	Ensure that safety glasses and hard hats are used

2)	Check where load will land should it slip, fall, or the lifting slings or chains fail

3)	Request that any untrained personal leave the area

4)	Ensure that a load is never lifted over any part of a person’s body or over people

5)	Check the stability of the lifting hoist.

The undersigned individuals have received and understood the safety training and have demonstrated proficiency in the operation of the 1000 kg Gantry Crane up to loads of 1000 kg.

Trainee Signature:					Date:

Instructor Signature:				Date: